* DELIVERY FILES SCANNED FORMATS:

Considering the need to download the files in question through the FTP site, maximum attention was given the choice of scanned formats.

Thus two binary formats were chosen in place of the ASCII formats that are much larger by nature.

Each format contains the 17 scanned files done already together with their related panorama photos done during the scanning sessions.

1. Format E57 : Useable by the majority of software used for managing data coming from Laser Scanners .

Two versions were prepared :

1. E57 100% ( maximum detail ) , size 8.69 GB
2. E57 75% ( reduced detail to guarantee a more compact file) , size 6.33 GB
3. Format RCP / RCS : Format Autodesk available for Software : Recap, Autocad 2014 and 2015, NavisWork , size 9.29 GB

To further compact the formats listed above, compressed files like ZIP have been prepared one for each format.

NB

The Recap program may be downloaded from internet and has almost all the functions activated for free